C:/Documents and Settings/frv128/Desktop/GIS Simulator v.1.5/Data/Test_
1.5
18-Aug-2009

# molecules []
1000000.000000
number of configurations
1.000000
angle between exit surface normal and center-origin extension, alpha1 [°]
0.000000
angle between exit center-origin extension and substrate normal, alpha2 [°]
60.000000
distance from tube exit surface center to substrate origin [r]
5.000000
tube length [r]
5.000000
tilt of plane cutting the tube [°]
0.000000
outer radius of the tube [r]
1.750000
hole?
0.000000
z position of "hole-"cylinder axis crossing the tube axis [r]
3.000000
tilt of "hole-"cylinder axis relative to tube axis [°]
0.000000
radius of "hole-"cylinder [r]
0.500000
transmission coefficient of "hole-"cylinder 
1.000000
freeflight?
1.000000
mean free path [r]
1.000000
pressure decay?
0.000000
total pressure decay along the tube in percent
10.000000
uptake coefficient (per tube collision!)
0.000000
gridsize
64.000000
imagesize [r]
12.000000
Number of virtual planes (including entrance and exit plane)
50.000000
Angular distribution histogram at x [px]
0.000000
Angular distribution histogram at y [px]
0.000000
Neighbours [px]
64.000000
Angle step for angular distribution histogram [°] (minimal 1°)
1.000000
seed 1
-964545310.000000
seed 2
-5416974.000000
seed 3
-110257687.000000
seed 4
-64335422.000000
end